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Here is the comparison about the tow maf transfer function the line blue is the 94-95 5.0 and the red one is the 88-93 5.0, i notice that they are very similar not the same but very closed, so what do you think about this table? It could be or not a problem using the 88-93 maf sensor in a 94-95 maf housing and viceversa? Or that little discrepancies can affect the performance in my 91 stang? 
